# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-04-29-153505

ClockPeriod(): 39390ns

measure period: 130s
network load: none
system load: none
time synchronization: PTP
PTP/NTP daemon priority: -25
edge_generator priority: -28
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
   [spirent_bi-directional]
   QNX + ptp master <-> switch <-> switch <-> QNX + ptp slave
                                          <-> spirent transceiver
                               <-> spirent transceiver

