# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-07-31-104600

ClockPeriod(): 39390ns

measure period: 130s
network load: none
system load: none
time synchronization: PTP (only master, because there is no ethernet connectivity on the QNX host)
PTP/NTP daemon priority: -25
edge_generator priority: -245
FitKit calibration: none

NOTE: master (the blue QNX box) RS232 was connected to the slave pin on FITkit

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
QNX host <-> FITkit
