# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-05-09-150844

ClockPeriod(): 39390ns

measure period: 1s
network load: 100% on NTP slave
system load:  cpu0 8% idle cpu1 93% idle
time synchronization: NTP
PTP/NTP daemon priority: -25
edge_generator priority: -28
FitKit calibration: none

ntpd was cca 17 minutes running

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
        QNX + ntp master <-> switch <-> QNX + ntp slave + receiver of spirent
                                                          dummy packets
                                    <-> spirent transmitter

