# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-07-30-131000

ClockPeriod(): 39390ns

measure period: 130s
network load: none
system load: none
time synchronization: PTP
PTP/NTP daemon priority: -25
edge_generator priority: -28
FitKit calibration: none

NOTE: master (the blue QNX box) RS232 was connected to the slave pin on FITkit

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
master <-> FITkit
