# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-04-25-151136

ClockPeriod(): 39390ns

network load: 100% on PTP slave (ICMP destination unreachable)
system load: CPU0 60%; CPU1 65%
time synchronization: PTP
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
    QNX + ptp master <-> switch <-> QNX + ptp slave + receiver of spirent
                                                      dummy packets
                                <-> spirent transmitter

