# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-04-25-125635

ClockPeriod(): 39390ns

network load: 100% on PTP master (ICMP destination unreachable); 0% on PTP slave
system load: none
time synchronization: PTP
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
    QNX + ptp slave <-> switch <-> QNX + ptp master + receiver of spirent
                                                      dummy packets
                                <-> spirent transmitter
