# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-04-25-172258

ClockPeriod(): 39390ns

network load: 100% on PTP slave; 0% on PTP master
system load: CPU0 94%, CPU1 4%
time synchronization: PTP
PTP/NTP daemon priority: -25
edge_generator priority: -25
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
    QNX + ptp master <-> switch <-> QNX + ptp slave + receiver of spirent
                                                      dummy packets
                                <-> spirent transmitter

