# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-04-24-164656

ClockPeriod(): 39390ns

network load: 100% throught cable both way
system load: none
time synchronization: PTP
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
    [spirent_bi-directional]
    QNX + ptp master <-> switch <-> switch <-> QNX + ptp slave
                                           <-> spirent transceiver
                                <-> spirent transceiver

