# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-05-08-150213

ClockPeriod(): 39390ns

measure period: 130s
network load: 100% through shared wire [NTP slave switch -> NTP master switch]
system load: none
time synchronization: NTP
PTP/NTP daemon priority: -25
edge_generator priority: -28
FitKit calibration: none

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
      [spirent_uni-directional]
      QNX + ptp master <-> switch <-> switch <-> QNX + ptp slave
                                             <-> spirent transmitter
                                  <-> spirent receiver

