# Topology specification (how many and which components, which
#   settings, which wiring...)
# measure: 2013-05-09-143418

ClockPeriod(): 39390ns

measure period: 1s
network load: 100% on NTP slave
system load: cpu0 8% idle cpu1 94% idle
time synchronization: NTP
PTP/NTP daemon priority: -25
edge_generator priority: -28
FitKit calibration: none

ntpd was running 13 minutes

!!!!!!!!!!!  WIRE TOPOLOGY  !!!!!!!!!!!
        QNX + ptp master <-> switch <-> QNX + ptp slave + receiver of spirent
                                                          dummy packets
                                    <-> spirent transmitter

